**Tender 2 - Holistic Summary Table**

*Generated on: Saturday, 1 November, 2025 at 7:33 pm*

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Tender ID** | **Tender Title** | **Issuing Authority** | **Submission Deadline** | **Tech Bid Opening** | **Price Bid Opening** | **Delivery Location** | **Delivery Schedule** | **AWPL Manufacturer Status** | **AWPL GST Status** | **AWPL Vendor Reg (PGVCL)** | **AWPL Factory License** | **AWPL ISO 9001:2015** | **AWPL Experience** | **AWPL Financial Turnover (FY23-24)** | **AWPL MSME Status** | **AWPL Gujarat Based** | **Tender SKU (Core Config)** | **Tender Insulation Type** | **Tender Rated Voltage** | **Tender Applicable Standards** | **Tender Conductor Material** | **Tender Insulation Thickness (Phase/Neutral)** | **Tender No. of Strands (Cond/Mess)** | **Tender Max DC Resistance (Phase)** | **Tender Tensile Strength (Alu/XLPE)** | **Tender Messenger Composition** | **Tender ISI Marking Req** | **AWPL Matched SKU Code** | **AWPL BIS License (Status/No.)** | **AWPL Type Test (Status/Date)** | **AWPL Prod Capacity (KM/yr)** | **Order Qty (KM)** | **Delivery Distance (KM)** | **Total Cost (Rs/km)** | **Economy Factor** | **Adjusted Cost (Rs/km)** | **Final Price (Rs/km)** | **Total Price (Rs)** |
| PGVCL/PROC/LT AB Cable/1228 | Procurement of LT Aerial Bunched Cables (XLPE Insulated) for LT Lines | Paschim Gujarat Vij Company Ltd. (PGVCL) | 10-Nov-2025 18:00 Hrs | 18-Nov-2025 11:00 Hrs | 03-Dec-2025 11:00 Hrs | Any of PGVCL stores in Gujarat (F.O.R. Destination) | 7 months on equal monthly basis, after 45 days from LOA | Yes (Works in India, GST Registered) | Valid (24AABCA1234F1Z5) | Valid (PGVCL/VR/2015/0847, until Mar 2027) | Valid (GL/FAC/2012/0891) | Valid (ISO/QMS/2014/0523) | Yes (Registered with PGVCL since 2015) | Rs. 58.90+ Crores | Not Registered (Medium Enterprise) | Yes (Vapi, Gujarat) | 1C x 35mm² + 1C x 16mm² + 25mm² messenger | XLPE | 1100V | IS-14255/1995, IS-8130/1984, IS-398/Pt.IV/1994, IS-10418/1982, IS-7098(Part-II):85 | Aluminum | Phase: 1.2mm / Neutral: 1.2mm | 7 / 7 | 0.868 Ohm/KM (Phase) | Alu: 90 N/mm² / XLPE: 12.5 N/mm² | Bare heat-treated Al-Si alloy (IS:398 Pt.IV), 7 strands, compacted | Mandatory on cable and drum | AW-ABC-1C-XLPE-35-16-25 | Valid (CM/L-9876543-C) | Valid (CPRI/TC/2021/4567, Mar 2021) | 3,200 KM/year (Single Core) | 1000 | 350 | 45254 | 0.925 | 41851 | 46873 | 46873000 |
| PGVCL/PROC/LT AB Cable/1228 | Procurement of LT Aerial Bunched Cables (XLPE Insulated) for LT Lines | Paschim Gujarat Vij Company Ltd. (PGVCL) | 10-Nov-2025 18:00 Hrs | 18-Nov-2025 11:00 Hrs | 03-Dec-2025 11:00 Hrs | Any of PGVCL stores in Gujarat (F.O.R. Destination) | 7 months on equal monthly basis, after 45 days from LOA | Yes (Works in India, GST Registered) | Valid (24AABCA1234F1Z5) | Valid (PGVCL/VR/2015/0847, until Mar 2027) | Valid (GL/FAC/2012/0891) | Valid (ISO/QMS/2014/0523) | Yes (Registered with PGVCL since 2015) | Rs. 58.90+ Crores | Not Registered (Medium Enterprise) | Yes (Vapi, Gujarat) | 3C x 35mm² + 1C x 16mm² + 25mm² messenger | XLPE | 1100V | IS-14255/1995, IS-8130/1984, IS-398/Pt.IV/1994, IS-10418/1982, IS-7098(Part-II):85 | Aluminum | Phase: 1.2mm / Neutral: 1.2mm | 7 / 7 | 0.868 Ohm/KM (Phase) | Alu: 90 N/mm² / XLPE: 12.5 N/mm² | Aluminum Alloy (IS:398 Pt.IV), 7 strands, compacted | Not explicitly mandatory for this config, but IS:14255/1995 applies | AW-ABC-3C-XLPE-35-16-25 | Valid (CM/L-9876544-C) | Valid (CPRI/TC/2022/5678, Aug 2022) | 2,800 KM/year (3C ≤35mm²) | 345 | 350 | 63479 | 0.961524164 | 61050 | 68376 | 23590920 |
| PGVCL/PROC/LT AB Cable/1228 | Procurement of LT Aerial Bunched Cables (XLPE Insulated) for LT Lines | Paschim Gujarat Vij Company Ltd. (PGVCL) | 10-Nov-2025 18:00 Hrs | 18-Nov-2025 11:00 Hrs | 03-Dec-2025 11:00 Hrs | Any of PGVCL stores in Gujarat (F.O.R. Destination) | 7 months on equal monthly basis, after 45 days from LOA | Yes (Works in India, GST Registered) | Valid (24AABCA1234F1Z5) | Valid (PGVCL/VR/2015/0847, until Mar 2027) | Valid (GL/FAC/2012/0891) | Valid (ISO/QMS/2014/0523) | Yes (Registered with PGVCL since 2015) | Rs. 58.90+ Crores | Not Registered (Medium Enterprise) | Yes (Vapi, Gujarat) | 3C x 50mm² + 1C x 25mm² + 35mm² messenger | XLPE | 1100V | IS-14255/1995, IS-8130/1984, IS-398/Pt.IV/1994, IS-10418/1982, IS-7098(Part-II):85 | Aluminum | Phase: 1.5mm / Neutral: 1.2mm | 7 / 7 | 0.641 Ohm/KM (Phase) | Alu: 90 N/mm² / XLPE: 12.5 N/mm² | Aluminum Alloy (IS:398 Pt.IV), 7 strands, compacted | Not explicitly mandatory for this config, but IS:14255/1995 applies | AW-ABC-3C-XLPE-50-25-35 | Valid (CM/L-9876544-E) | Valid (CPRI/TC/2023/6789, Jun 2023) | 1,800 KM/year (3C ≥50mm²) | 1500 | 350 | 78662 | 0.91 | 71582 | 80172 | 120258000 |